|  |  |
| --- | --- |
|  | **Injury & Illness Prevention Program**  Job Safety Analysis Form |
| 1000 E Victoria St.• Carson, CA 90747  Phone: 310-243-3000 • Office: 310-243-3171  www.csudh.edu/ehs |

|  |  |  |  |
| --- | --- | --- | --- |
| **Picture of task/equipment:** | **Task:** | Pressure Washing | |
|  | **Name of Shop or Dept:** | CSUDH Campus - Maintenance | |
| **Job Title(s):** |  | |
| **Analyzed by:** | M. Williams | |
| **Date:** | 10/1/2021 | |
| **Required PPE:** | | | |
| |  |  |  |  |  |  | | --- | --- | --- | --- | --- | --- | | **Slip-Resistant Boots** | **Gloves** | **Hearing Protection** | **Safety Glasses** | **Safety Vest** | **Mask/Face Protection** | | [http://i.pgcdn.com/pi/78/99/15/789915284_260.jpg](http://www.google.com/url?sa=i&rct=j&q=shoes+for+crews+boots&source=images&cd=&cad=rja&docid=DOgZc1yr_Rm1KM&tbnid=-1pgrn4msHdUpM:&ved=0CAUQjRw&url=http://shopping.yahoo.com/789915284--guardian-iii-steel-toe-black-non-skid-steel-toe-boots-and-shoes/&ei=qekjUdmXDuXZigLJ2YDgCw&bvm=bv.42661473,d.cGE&psig=AFQjCNGg-wPXvVaydGd2g1NKLJc4P6e-mQ&ust=1361394444673608) | Milwaukee Men's Cut 1 Nitrile Utility Gloves — Red/Black, Large, Model#  48-22-8902 | [http://www.homesafetymatters.com/product.img?cono=006&img=images/products/hires/earplug2.jpg&width=600&height=600](javascript:swapimage('http://www.homesafetymatters.com/product.img?cono=006&img=images/products/hires/earplug2.jpg&width=600&height=600')) | Mcr Safety | Safety Glasses: Anti-Scratch, No Foam Lining, Wraparound Frame, Half-Frame, Black, Black Model: SS110 |  | [Nuisance Removal Dust Mask, PK 50](javascript:%20void(0)) | |  |  |  |  |  |  | | | | |
| **Required/Recommended Trainings:** | | | |
|  | | | |
| **TASK** | **HAZARDS** | | **CONTROLS** |
| Pressure washing with a Hotsy or Landa Washer | **Slips**  **Trips**  **Falls**  **Lacerations**  **Struck-by**  **Electrocution** | | **Don** booties and place wet floor signs in direct area before operating a pressure washer.  **Use** a safety vest when there is risk of vehicular traffic in the area.  **Safety** glasses shall be worn to prevent particles from flying up and coming in contact with eyes.  **Be** familiar with how to turn off machine and bleed pressure out before operating the equipment.  **Make** sure electrical connections are grounded using a 3-prong outlet.  **Keep** water spray away from electric wiring or electric shock may result.  **Always** hold the spray gun with both hands to prevent kick back.  **Firmly** grip spray gun before starting to prevent gun from whipping and causing bodily harm.  **Never** spray washer towards persons or vehicles as it can cause bodily harm.  **Do not** attempt to overreach or stand on an unstable footing while operating equipment.  **Never** leave equipment unattended. |